BENDIGO-OPHIR GOLD PROJECT
PROPOSED CONSENTS AND CONDITIONS FOR RESOURCE CONSENTS WITHIN THE JURISDICTION OF THE OTAGO REGIONAL COUNCIL
UPDATED 28 AUGUST 2026

The base version of the following conditions is the version of the conditions dated 22 June 2026 that was provided to the EPA and Expert Panel following the Concurrent Hearings in Wellington.  
All additional changes made during the four conditions workshops held in July and August 2026 with planning experts from Otago Regional Council, Central Otago District Council, the Department of Conservation and Kā Rūnaka are presented in track changes.
The conditions shaded in light grey wash are where some of the parties have not had sufficient time to fully consider the proposed amendments including as a result of gaining technical advice (with any final comments expected to be provided by 7 September 2026).
Comments are included for some conditions to provide further context / clarification for changes made (where appropriate), to record points of disagreement between MGL and one or more parties, and to identify conditions where discussion between MGL and parties are in progress and are expected to be resolved by 14 September 2026.
These track changed conditions do not have updated numbering and cross-references (refer to the clean version where this has been updated).  
Notes:
All of the following consents are subject to compliance with:
The Common Conditions between the Central Otago District Council and the Otago Regional Council in Schedule One; and
The General Conditions in Schedule Two which apply to all Otago Regional Council consents.
Particular controls, limits, management of effects and monitoring required associated with the activities that are the subject of the consents below are controlled by way of the conditions in Schedules One and Two noted above.  On that basis, and to avoid unnecessary repetition, most of the following consents have relatively few individual conditions.  
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[bookmark: _Toc238479991]Section 9 Permits
	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S9
	A Land Use Consent to undertake earthworks, soil disturbance and vegetation clearance activities within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions for the purpose of mining development, mining operations, maintenance and ancillary activities, including locations within, or within a 10 m or 100 m setback from, natural inland wetlands within the catchments of Shepherds Creek, Rise and Shine Creek and an unnamed tributary of Clearwater  Creek that result in, or will likely result in, the complete or partial drainage of all or part of a wetland.

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.





	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S9
	A Land Use Consent to drill bores and holes associated with mineral exploration, geotechnical investigations, establishment of underground mine declines and drives to access and mine an ore body, blasting and dewatering activities and for the establishment of groundwater production and monitoring bores / piezometers within the area shown on Plan 2 – BOGP Consent Area annexed as part of Attachment 1 – Plans to the Common Conditions.

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.

	General Requirements – Bendigo Aquifer Borefield
Advice Note: The following conditions apply to bores associated with the taking of groundwater from the Bendigo Aquifer.  They do not apply to holes drilled for blasting, geotechnical dewatering and mineral exploration purposes.

	3
	The Otago Regional Council must be notified in writing at least 10 working days in advance of the installation of each bore, piezometer and groundwater monitoring bore.

	4
	The bore must be constructed and maintained so that it will not cause cross contamination between hydraulic units (aquifers) in any water (including groundwater).

	5
	All openings to the bore must be sealed or screened to prevent the entry of foreign matter or contaminants.  The ground immediately surrounding the top of the bore casing must be sealed and graded to drain surface water away from the bore.

	6
	Upon completion of the bore, any wastes introduced to the bore during drilling and construction must be removed.

	7
	If artesian conditions are encountered, a conductor casing must be grout sealed to ensure control of potential flowing artesian groundwater and to prevent instability of the ground at the bore head. Bore head completion must be such that groundwater leakage under flowing artesian pressures is prevented.

	8
	Discharge of wastewater from bore installation into or onto the ground is permitted provided that only non-hazardous and non-toxic drilling fluids and/or foams are used as approved by Otago Regional Council.  Drilling must be undertaken in such a manner that there is no discharge of grease or oil, and wastewater does not directly enter surface water.

	9
	Bores that are no longer operational must be decommissioned to prevent contamination, by grouting and capping.

	10
	The Consent Holder must submit to the Otago Regional Council, as part of the Annual Monitoring and Compliance Report, a report which contains:
(a) A log for each bore drilled during that calendar year. Each log must show: 
(i) The location of the bore; in NZTM2000 coordinates;
(ii) Date of completion;
(iii) Duration of drilling;
(iv) Depth and diameter of the bore;
(v) The method of drilling;
(vi) Full construction details; 
(vii) The subsurface geology; 
(viii) Development information; and
(ix) Installed instrumentation (pumps, loggers, flow meters etc.).
(b) A list of any decommissioned bores, including their logs.




[bookmark: _Toc238479992]Section 13 Permits
	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S13
	A Land Use Consent to place, use, maintain, upgrade and remove structures in the beds of watercourses and in natural inland wetlands within the catchments of Shepherds Creek, Rise and Shine Creek and an unnamed tributary of Clearwater Creek associated with mine development, operation, maintenance and closure activities within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.

	Design and Performance Requirements – All Instream Structures

	NEW 1
	No less than 15 days prior to the commencement of works for the installation of any instream structure, the Consent Holder must advise Otago Regional Council of the intended works commencement date. 

	3
	The culverts in the Rise and Shine Creek must be located in general accordance with the Plan in Attachment 1 to this consent and be constructed and operated to convey the runoff resulting from at least a 5% Annual Exceedance Probability (“AEP”), 24-hour duration, design storm for all durations.

	4
	The Consent Holder must ensure that the area of disturbance during placement / construction of all instream structures is kept to a practical minimum and is undertaken in accordance with a Site-Specific Erosion and Sediment Control Plan (“SSECP”) as required by Condition 2 of the Schedule 2 General Conditions which apply to all of the resource consents within the jurisdiction of the Otago Regional Council.

	NEW 2
	The Consent Holder must undertake routine monitoring and maintenance of the culverts (once placed), as detailed below:
(a) Engage a Suitably Qualified and Experienced Person (“SQEP”) to  The Consent Holder must visually inspect each culvert within five days of any event that may cause damage that could affect the culvert’s stability, the ability of the culvert to provide sion for fish passage, ability to convey the design flows, or cause erosion or scour; and
(b) If any of the visual inspections in clause (a) identify that the culvert is damaged, engage a Suitably Qualified and Experienced Person (“SQEP”) to assess the damage and provide recommendations to remedy the damage.  The Consent Holder must then undertake the recommended repair and / or maintenance works as soon as practicable to remedy the issues identified.
Following any maintenance works undertaken in accordance with clause (b) of this condition, provide to the Consent Holder an updated version of the information relating to the structure as set out in Condition 5 of this consent.
Advice Note: For the avoidance of doubt, the various technical assessments prepared as part of the Substantive Application demonstrated that the water bodies within the Project Site do not contain any fish species.

	5
	Consent Holder must provide the Otago Regional Council with the information required under Regulations 62(3) and 63(3) of the Resource Management (National Environmental Standards for Freshwater) Regulations 2020 (“NES Freshwater”) no more than 20 working days following completion of the installation of the culverts within Rise and Shine Creek.
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Attachment 1 – Location of Culverts in the Rise and Shine Creek	Comment by Mitchell Daysh: FYI - new plan added to show two new culverts in RAS Creek associated with new lizard sanctuary.
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	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S13
	A Land Use Consent to alter, disturb and reclaim the beds of the Shepherds Creek, Rise and Shine Creek, Jean Creek and an unnamed tributary of Clearwater Creek, including associated tributaries and connected natural inland wetlands within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	




	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.





[bookmark: _Toc238479993]Section 14 Permits
	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S14
	A Water Permit to: 
Take and use groundwater from the Bendigo Aquifer for the purposes of supplying water to support all mining construction, operation, maintenance and ancillary activities (including ecological rehabilitation and enhancement) and for augmenting flows within Shepherds Creek, Rise and Shine Creek and natural inland wetlands; and
Take groundwater for dewatering purposes associated with open pit and underground mining operations;
within the Project Site shown on Plan 1 - Project Overview Plan and the BOGP Consent Area shown on Plan 2 – BOGP Consent Area annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).  Consent Area annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.

	Water Take from the Bendigo Aquifer

	3
	The maximum instantaneous rate of take from the production bores must not exceed 110 97 litres per second.	Comment by Mitchell Daysh: FYI -  Amended in accordance with the findings of the RFI 11 responses.

	NEW 3
	Prior to commencing operational use of the bores, the Consent Holder must:	Comment by Mitchell Daysh: Deleted as works undertaken as part of RFI 11.
(a) Undertake an aquifer test in accordance with the Otago Regional Council Aquifer Test Guidelines, as detailed in Attachment 1; and
(b) Engage a suitably qualified and experienced hydrogeologist to interpret the aquifer test data to predict the extent of drawdown at other bores (that are used for abstractive purposes) within the aquifer; and
(c) If the findings of (b) are that the drawdown is of a magnitude that is likely to interfere with that bore operation, the Consent Holder must implement the process described in Condition NEW 3.

	4
	The Consent Holder must install a system to measure on a continuous basis the volume taken via the bore. The system must have a reliable calibration and must be maintained to an accuracy of +/- 5 percent.

	5
	Within one month of installation of the system required by Condition 4, the Consent Holder must provide Otago Regional Council:
(a) A copy of any relevant manufacturer calibration certificate; and
(b) Evidence from a suitably qualified person showing that the system required by Condition 4 is verified as accurate to +/- 5 percent.

	6
	The Consent Holder must engage a suitably qualified person to undertake additional verification of the accuracy of the system required by Condition 4:
(a) At the written request of Otago Regional Council; and
(b) At a frequency of no less than five yearly from the date of the first verification required by Condition 4; and
(c) To the satisfaction of Otago Regional Council.
Evidence documenting each additional verification must be forwarded to Otago Regional Council within one month of the verification being completed.

	7
	The Consent Holder must telemeter – via a telemetry system developed after liaison with Otago Regional Council to ensure that the telemetry system is compatible with Otago Regional Council telemetry system standards and data protocols - continuous 15-minute values of take volume (in units of cubic metres).  The data must be reported once daily to Otago Regional Council via the telemetry system and there must be 96 values per parameter per daily report.  When no groundwater is being taken the data must specify the take volume as zero.

	NEW 4
	The Consent Holder must ensure the full operation of the water measuring system and telemetry unit at all times during the exercise of this consent. All malfunctions of the water measuring or telemetry unit during the exercise of this consent must be reported to the Otago Regional Council within 5 working days of observation.  Appropriate repairs must be performed within 30 working days of observation of the malfunction or within a timeframe agreed with the Otago Regional Council.
Once the malfunction has been remedied, a copy of the calibration record, Water Measuring Device Verification Form (Form RS1) with photographic evidence and any non-transferred data must be submitted to the Otago Regional Council within 5 working days of the completion of repairs. 
Photographs must be in colour and be no smaller than 200 x 150 millimetres in size and be in JPEG form.
Advice Note:  The water meter, data logger and telemetry unit should be safely accessible by the Otago Regional Council and its contractors at all times. The Water Measuring Device Verification Form and Calibration Form are available on the Otago Regional Council’s website.

	NEW 5
	In the event that the cumulative drawdown assessment required by Condition NEW 1 indicates avulnerability to project-induced drawdown and difficulties to the pumping operation of a surrounding water bore, the Consent Holder must:	Comment by Mitchell Daysh: Condition deleted with new amended version below to reflect the RFI 11 response and address the concerns raised by Hayden Johnston (The Canyon Vineyard Ltd (Tarras Vineyards)) in his comments for consideration at the conditions workshops.
(a) Undertake a follow-up consultation and a request to investigate remedial actions with the affected bore owner;
(b) Undertake investigations which may include:
(i) Detailed measurements of the affected bore(s);
(c) Reference to bore log, bore construction and drilling records;
(d) Pulling the pump unit and making essential measurements; and
(e) Measuring the internal decline in bore water level during pumping of the subject bore (specific capacity or step rate testing); and
(f) Investigate potential remedial actions, which may include:
(i) Lowering of the pump unit within the original bore (where feasible);
(g) Re-drilling of the bore and setting a deeper, larger diameter screen so as to allow lower setting of the pump unit and higher screen loss efficiency;
(h) Provision of a replacement, high reliability water supply of equal or better water quality in the case of elevated risk of bore water supply interruption that cannot be remedied by any other means; and
(ii) Consult the affected bore owner and implement the most practicable and effective remedial option to ensure that the bore owner can continue to access and abstract water at the rate and volume that that they were abstracting prior to the commencement of the BOGP, taking into account any preferences of the bore owner about the solution to be implemented.

	NEW 5
	Within 30 working days following the commencement of this consent, the Consent Holder must notify the owners of groundwater bores within 1 km radius of the Bendigo Aquifer bore CB13/0215 (the subject of this consent) of the anticipated commencement date for which groundwater will be first taken, and invite those surrounding bore owners to provide the following information in relation to their existing lawfully established bores / water takes:
(i) Location and depth of the bore;
(j) Standing depth to water;
(k) Consented rate and volume of water take (including any seasonal variations);
(l) A description of the physical infrastructure associated with the take (e.g. submersible pump, surface pump, any water conveyance infrastructure etc.); and
(m) A copy of any resource consents (where applicable). 
All surrounding bore owners who provide the information above within 30 working days of the date of the request will be eligible to benefit from the regime set out in Condition NEW 5A below.

	NEW 5A
	If any surrounding bore owner that has provided the information set out in accordance with the requirements set out in Condition NEW 5 advises the Consent Holder that they cannot access their full consented or permitted allocation of groundwater, the Consent Holder must then undertake the following sequential steps:
(a) The Consent Holder must commission an independent hydrogeological assessment to verify the alleged issues with accessing their full groundwater allocation and likely causes to determine whether this reduction is caused by the Consent Holders take at the Bendigo Aquifer authorised by this consent.  This assessment must be prepared by a SQEP and provided to ORC and the affected bore owner with 40 working days.
(b) If the assessment required in clause (a) concludes that the reported issues with accessing their full allocation are a result of the Consent Holders take at the Bendigo Aquifer authorised by this consent, the Consent holder must provide an alternative water supply equivalent to the confirmed shortfall until the following steps have been completed:
(i) Undertake investigations which may include (but are not limited to):
1) Detailed measurements of the affected bore(s);
2) Reference to bore log, bore construction and drilling records;
3) Pulling the pump unit and making essential measurements; and
4) Measuring the internal decline in bore water level during pumping of the subject bore (specific capacity or step rate testing).
(ii) Investigate and implement the most practicable and effective remedial option to ensure that the bore owner can continue to access and abstract water at the rate and volume that that they were abstracting prior to notification of the reported drawdown, taking into account any preferences of the bore owner about the solution to be implemented.  These solutions may include, but are not limited to, the following:
1) Lowering of the pump unit within the original bore (where feasible);
2) Re-drilling of the bore and setting a deeper, larger diameter screen to allow lower setting of the pump unit and higher screen loss efficiency; or
3) Provision of a replacement, high reliability water supply of equal or better water quality in the case of elevated risk of bore water supply interruption that cannot be remedied by any other means.
Advice Note:  If the affected bore owner is abstracting water in accordance with a permitted activity rule that has a fixed limit, the Consent Holder must ensure that the full volume allowed for by that permitted activity rule is accessible by the affected bore owner.





Attachment 1 – Otago Regional Council Aquifer Test Guidelines
To be attached to final version:
https://www.orc.govt.nz/media/14441/aquifer-test-guidelines.pdf 



	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S14
	A Water Permit to dam, divert, take and use surface water from the Shepherds Creek, Rise and Shine Creek, Jean Creek and associated tributaries and an unnamed tributary of Clearwater Creek, and from the RAS, CIT, SRX and SRE Open Pits, for the purposes of mining construction, operation, maintenance and ancillary activities including locations within, or within a 10m or 100m setback from, natural inland wetlands that results in, or is likely to result in, the complete or partial drainage of all or part of the wetland within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.





[bookmark: _Toc238479994]Section 15 Permits
	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S15
	A Discharge Permit to discharge water and associated contaminants to water associated with: 
The discharge of water (taken from the Bendigo Aquifer) into Shepherds Creek and Rise and Shine Creek for the purpose of augmenting flows;
The discharge of water and associated contaminants from the SRX Open Pit, SRX ELF and portions of the Western ELF and RAS Open Pit into Rise and Shine Creek; 
The discharge of water and associated contaminants from the Western ELF into an unnamed tributary of Clearwater Creek;
The discharge of water and associated contaminants from the Shepherds Silt Pond to Shepherds Creek (in the form of the Shepherds Stream Diversion); 
The discharge of water and contaminants from erosion and sediment control structures in accordance with certified Site-Specific Erosion and Sediment Control Plans; and
The discharge of treated mine water from the water treatment plant (or passive treatment system) and associated contaminants to Shepherds Creek during mine closure;
within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.

	Augmentation of Flows in the Shepherds Creek and Rise and Shine Creek

	3
	Maintenance of Flows
(a) Within six months of the commencement of these consentsPrior to any land disturbance activities that may result in the depletion of flows in Rise and Shine Creek and Shepherds Creek, the Consent Holder must commence stream augmentation to maintain the mean monthly surface water flow rates at Rise and Shine Creek and Shepherds Creek.
(b) The flows in Rise and Shine Creek and Shepherds Creek must be maintained at the estimated pre-mining influenced mean monthly surface flow rates detailed below by, if necessary, augmenting flows in Shepherds Creek and Rise and Shine Creek using water taken from the Bendigo Aquifer under Water Permit [insert consent number].  
	Month
	SC01
	RS03

	January
	10.8
	8.1

	February
	7.0
	5.3

	March
	6.6
	5.0

	April
	7.6
	5.7

	May
	12.8
	9.7

	June
	21.9
	16.5

	July
	32.1
	24.2

	August
	39.7
	29.9

	September
	31.8
	24.0

	October
	21.7
	16.4

	November
	24.4
	18.4

	December
	14.3
	10.8


Note: all values are litres per second.
Advice Note: For the purposes of this condition, land disturbance activities that may result in stream depletion include open pit development, stream reclamations and damming and diversion activities.

	
	Augmentation must be undertaken in general accordance with the Flow Augmentation Strategy Memorandum prepared by Hydro Geochem Group Limited dated 20 October 2025 (HGG 2025b), included in the application as Report B.43.  
Augmentation of Flows
Subject to adjustments as described in Condition 3(c) below, the Consent Holder must undertake, as a minimum, surface water augmentation of the Rise and Shine Creek and Shepherds Creek at the flow augmentation sites (shown in Attachment 1 to this consent) shall require as a minimum surface water augmentation at the following to maintain the flows rates in Condition X above.:  
	Month
	SC01
	RS03

	
	SW
	GW
	TOTAL
	SW
	GW
	TOTAL

	January
	2.9 (-27%)
	3.5
	6.4
	0.6 (-7.5%)
	2
	3.2

	February
	1.9 (-27%)
	3.5
	5.4
	0.4 (-7.5%)
	2
	2.8

	March
	1.8 (-27%)
	3.5
	5.3
	0.4 (-7.5%)
	2
	2.7

	April
	2.0 (-27%)
	3.5
	5.5
	0.4 (-7.5%)
	2
	2.9

	May
	3.5 (-27%)
	3.5
	7.0
	0.7 (-7.5%)
	2
	3.5

	June
	3.7 (-17%)
	3.5
	7.2
	1.1 (-6.5%)
	2
	4.1

	July
	5.5 (-17%)
	3.5
	9.0
	1.6 (-6.5%)
	2
	5.1

	August
	6.7 (-17%)
	3.5
	10.2
	1.9 (-6.5%)
	2
	5.9

	September
	5.4 (-17%)
	3.5
	8.9
	1.6 (-6.5%)
	2
	5.1

	October
	3.7 (-17%)
	3.5
	7.2
	1.1 (-6.5%)
	2
	4.1

	November
	4.1 (-17%)
	3.5
	7.6
	1.2 (-6.5%)
	2
	4.4

	December
	3.9 (-27%)
	3.5
	7.4
	0.8 (-7.5%)
	2
	3.6



Note: All figures are reported in litres per second, unless otherwise stated. SW reductions represent those as a result of changes in catchment areas and changes to runoff processes. GW reductions are from dewatering of RAS and CIT pit voids and underground workings.

	
	Augmentation Flow Rate Increase
(c) Subject to adjustments as described in Condition 3(f). below, the Consent Holder must increase augmentation flow rates in addition to those required in Condition 3(b above upon the commencement of the below identified mine domains components below:
(i) For Shepherds Creek (SC01):
1. 10.0 litres per second for all months once the RAS Underground commences; and
2. 1.7 litres per second for all months once the CIT Open Pit commences. 
(ii) For Clearwater / Rise and Shine Creek (RS03):
1. 15.3 L/s for all months once the SRX Open Pit commences.
The discharge sites for augmented flows must be located upstream of all water takes associated with the BOGP, in general accordance with Sites 1, 2, and 3 as described in HGG 2025, and as shown in Attachment 1 of this consent;

	
	Monitoring and Reporting 
The Consent Holder will must implement the following performance monitoring methods to ensure the rate of augmentation is appropriate to ensure surface creek flows are maintained at the estimated pre-mining influenced mean monthly surface flow rates identified in Condition 3a above:
(i) Record volumes and flow rates of water discharged for flow augmentation;
(ii) Install automated creek flow gauging sites at:
1. RS03 on Clearwater Creek to monitor flow changes in Clearwater Creek and Rise and Shine Creek;
2. An additional site on Clearwater Creek upstream of the confluence with Rise and Shine Creek to distinguish natural flow variability from mine influence; and
3. SC01 to monitor flow changes in Shepherds Creek.
(iii) Install groundwater level monitoring at selected locations to provide early warning of creek flow losses due to drawdown;
(d) If performance monitoring data at the automated creek flow gauging sites shows augmentation flow rates are too high, or too low, relative to the minimum mean monthly flow rates specified in Condition 3a above, the Consent Holder must adjust the augmentation flow rates accordingly in order to maintain the mean monthly surface flow rates at Rise and Shine Creek and Shepherds Creek as set out in Condition 3a above; and 
This condition does not apply in the post-closure phase once performance monitoring demonstrates creek flows exceed pre-mining flows without any augmentation.

	Active Water Treatment Plant

	NEW 6
	Water Treatment Studies
Within one year of tailings being produced, the Consent Holder must commission water treatment studies which utilise representative mine impacted waters to inform the detailed design of the Active Water Treatment Plant.  The water treatment studies must include, at a minimum:
(a) A review of literature to validate preferred treatment processes;
(b) Bench testing - simulation of each step in the treatment train;
(c) Scaled-up testing / pilot trials as necessary to ensure the process works at the required scale;
(d) Assessment of mine impacted water sludge or processing residues to inform the appropriate management requirements once treatment commences; and
The water treatment studies Must must be informed by:
(a)  tThe results of the cover system trials required by Condition 20; and
(e) Must be informed by tThe wWater lLoad and bBalance mModelling required by conditions to ensure that the aActive wWater tTreatment pPlant is designed with adequate capacity.
For each year that the water treatment studies are undertaken, Tthe Consent Holder must include the results (and any associated analysis or interpretation) of all testing that is carried out in accordance with this condition in the Annual Compliance and Monitoring Report required by Common Condition C12, and details on work proposed for the next 12 months within the Annual Work Programme required by Condition C11 of the Common Conditions which apply to all of the resource consents within the jurisdiction of the Central Otago District Council and Otago Regional Council.

	NEW 7
	No less than three months prior to commencing construction of the Active Water Treatment Plant, No later than four years after tailings are first produced, the Consent Holder must submit to Otago Regional Council for certification the detailed design for the Active Water Treatment Plant.  The detailed design must be prepared by a Suitably Qualified and Experienced Person (“SQEP”) and must be informed by the results of the water treatment studies required under Condition NEW 6.

	NEW 7A
	The Active Water Treatment Plant must be designed to achieve the following standards and requirements:
(a) All discharges from the plant will achieve the surface water quality compliance limits set out in Attachment 5 of Schedule Two at the discharge point;
(b) The plant must be located outside of the 1% AEP flood level;
(c) The plant must be designed to include safeguards to minimise the risk of physical failure of the plant and to avoid or minimise adverse effects on the receiving environment in the event of a failure; and
The plant must be designed to include safeguards to minimise the risk of treatment process failure and to avoid or minimise adverse effects on the receiving environment in the event of a failure.

	NEW 8
	The Consent Holder must instigate the construction and subsequent commissioning of the Active Water Treatment Plant where monitoring indicates a sustained and attributable need to avoid adverse effects on receiving environments.  This requirement is triggered upon the earliest occurrence of any of the following triggers:
Persistent deterioration in surface water quality (defined by the advice note below) at compliance monitoring locations attributable to mine-related runoff;  
(b) Measured sulfate concentrations at groundwater performance monitoring sites GW02A, GW02B and GW02C (shown on Attachment 3 – Groundwater Monitoring Locations and listed in Attachment 4 – Groundwater Monitoring Location Details in the General Conditions in Schedule Two (that apply to all of the resource consents within the jurisdiction of ORC) which exceed 50% of the applicable compliance limit on three occasions within 12 months, including at least one exceedance of the limit, that is attributable to activities on the Project Site and cannot be remedied through adaptive management processes; or 
(a) Development of a water surplus condition that is not being adequately managed by engineering controls, as predicted by water load balanceing modelling where mine circuit water requires discharge (as set out in Conditions 29-33 of the of the Schedule 2 General Conditions which apply to all of the resource consents within the jurisdiction of the Otago Regional Council); and or
(b) Permanent cessation of mining where ongoing water management is required.
Following confirmation of a trigger that a trigger has been reached, the Consent Holder must:
(c) Notify the Otago Regional Council within 20 working days; and  
(d) Subject to Condition NEW 6, construct and commission the Active Water Treatment Plant as soon as reasonably practicable, and no later than 12 months after the trigger is confirmed has been reached, unless otherwise agreed between the Consent Holder and Otago Regional Council.
Advice Note: Surface water deterioration is where measured sulfate concentrations, a key indicator of mine impacted water, at compliance monitoring locations exceeds 50% of the applicable compliance limit on three occasions within 12 months, including at least one exceedance of the limit, where attributable to site activities and not resolved by adaptive management processes.

	NEW 9
	The water discharged from the Active Water Treatment Plant must at all times comply with the surface water compliance limits shown in Attachment 25 of the General Conditions which apply to all of the resource consents within the jurisdiction of the Otago Regional Council.

	Monitoring and Reporting

	NEW 10
	The Consent Holder must undertake the following sampling requirements will be required during the operational phase of the Active Water Treatment Plant:
(a) Online (Realtime) continuous monitoring of pH, Tturbidity and EC electrical conductivity of treated water should be included the water treatment plant instrumentation.  These should which must be calibrated daily by the water treatment plant operations staff; and
(b) Weekly Monthly water quality analysis of total and dissolved metals by an IANZ accredited laboratory of all surface water quality compliance parameters shown in Attachment 25 of the General Conditions in Schedule Two the General Conditions (which apply to all of the resource consents within the jurisdiction of the Otago Regional Council) by an IANZ accredited laboratory should be carried out at the discharge point from the Active Water Treatment Plant treated water polishing pond.
The Consent Holder must provide a summary of the monthly water quality results (and any associated analysis or interpretation) carried out in accordance with clause (b) in the Annual Compliance and Monitoring Report required by Common Condition C12 in Schedule One.

	NEW 11
	The Consent Holder must develop Aan Operations and Maintenance Manual will be developed for the Active Water Treatment Plant prior to the operation of the plant going operational.  This will must include, as a minimum, the following:
(a) Alarms response procedures;
(b) Maintenance Schedules;
(c) Sampling Requirements;  
(d) Calibration;
(e) Performance testing requirements;
(f) Manufacturers data and manuals;
(g) Material Safety Data Sheet (“MSDS”) information;
(h) Change management; and 
(i) Hazardous Substances and New Organisms Act 1996 (“HSNO”) Requirements.; 
(j) Processes for the removal and disposal of water sludge or processing residues, including frequencies and triggers; and
(k) Contingency measures in the event of engineering or process failure at the plant.

	Passive Water Treatment System

	NEW 12
	Water Treatment Studies
The Consent Holder must undertake studies to confirm that the Passive Water Treatment System will meet the water quality limits set out in Attachment 25 of Schedule Two during post closure.  Specifically:
(a) For passive treatment in Shepherds Creek, the studies are required to commence at least 5 years before passive treatment is required and within 5 years of active treatment commencing; and
(b) For passive treatment Rise and Shine Creek, the studies are required to commence at least 5 years before passive treatment is required., noting that the SRX Open Pit is anticipated to spill within 6 months of dewatering ceasing.
The passive water treatment studies must include, at a minimum:
(a) A review of literature to validate preferred treatment processes;
(b) Bench testing - simulation of each step in the passive treatment train;
(c) Scaled-up testing / pilot trials as necessary to ensure the passive treatment process works at the required scale; and
(d) Assessment of mine impacted water sludge to inform the appropriate management requirements once treatment commences.
The passive water treatment studies must be informed by:
(a) The results of the cover system trials required by Condition 20 (ELF Cover Trials in D.04); and
(b) The Water Load and Balance modelling required by conditions X to ensure that the Passive Water Treatment System is designed with adequate capacity.

	NEW 13
	For each year that the water treatment studies are undertaken, Tthe Consent Holder must include the results (and any associated analysis or interpretation) of all passive water treatment studies undertaken in accordance with Condition NEW 12 [above] in the Annual Compliance and Monitoring Report required under Common Condition C12 in Schedule One, and details on work proposed for the next 12 months within the Annual Work Programme required by Common Condition C11 of the Common Conditions which apply to all of the resource consents within the jurisdiction of the Central Otago District Council and Otago Regional Council in Schedule One.

	NEW 14
	No less than three months prior to commencing construction of the Passive Water Treatment System, the Consent Holder must submit the detailed design for the Passive Water Treatment System to Otago Regional Council for certification (including being reviewed by the Peer Review Panel as detailed in Condition CX of the Common Conditions in Schedule One).
The detailed design must be prepared by a SQEP and must be informed by the results of the water treatment studies required under Condition NEW 12.
Advice Note: Criteria must be prepared by a SQEP and must be informed by outcomes of the testing condition in Condition NEW 6.

	NEW 14A
	The Passive Water Treatment System must be designed to achieve the following standards and requirements:
(a) All discharges from the system will achieve the surface water quality compliance limits set out in Attachment 5 of Schedule Two at the discharge point;
(b) The system must be located outside of the 1 in 100-year Annual Reoccurrence Interval (“ARI”) event;
(c) The system must be resilient to extreme weather events (taking into account the expected effects of climate change);
(d) The system must be designed to include safeguards to minimise the risk of physical failure and to avoid or minimise adverse effects on the receiving environment in the event of a failure; and
(e) The system must be designed to include safeguards to minimise the risk of treatment process failure and to avoid or minimise adverse effects on the receiving environment in the event of a failure.

	NEW 15
	The water discharged from the Passive Water Treatment System must at all times comply with the surface water compliance limits shown in Attachment 2 of the Schedule Two General Conditions (which apply to all of the resource consents within the jurisdiction of the Otago Regional Council).

	
	Monitoring and Reporting

	NEW 16
	The Consent Holder must undertake the following sampling requirements during the operational phase of the passive water treatment system:
(a) Online (Realtime) continuous monitoring of pH, dissolved oxygen, and electrical conductivity of treated water; and
(b) Weekly Monthly water quality analysis of total and dissolved metals by an IANZ accredited laboratory of all the surface water quality compliance parameters shown in Attachment 25 of the General Conditions in Schedule Two (which apply to all of the resource consents within the jurisdiction of the Otago Regional Council) by an IANZ accredited laboratory at the discharge point of the Passive Water Treatment System.  The sampling frequency may decrease to monthly once confidence in electrical conductivity relationships have been developed if agreed with ORC.	Comment by Mitchell Daysh: FYI - Changed to monthly in accordance with changes to Active Water Treatment Plant conditions.
The Consent Holder must provide a summary of the monthly water quality results (and any associated analysis or interpretation) carried out in accordance with clause (b) in the Annual Compliance and Monitoring Report required by Common Condition C12 in Schedule One.

	NEW 17
	The Consent Holder must develop an Operations and Maintenance Manual for the passive water treatment system prior to the operation of the system becoming operational.  This must include, as a minimum, the following:
(a) Maintenance Schedule;
(b) Monitoring requirements and processes;
(c) Data management;
(d) Change management;
(e) Health and safety requirements;
(f) Processes for the removal and disposal of water sludge or processing residues, including frequencies and triggers; and
(g) Contingency measures in the event of engineering or process failure of the system.




Attachment 1 – Flow augmentation sites
[image: ]
	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S15
	A Discharge Permit to discharge water and contaminants to land, including circumstances where contaminants may enter water, associated with:
The discharge of soil and rock material to create the various topsoil and brown rock stockpiles, the TSF, various ELFs, the Shepherds Service Corridor, haul roads, erosion and sediment control structures and treatment devices, two aggregate pits, and to support the construction of any ancillary mining development, operation and maintenance activities;
The discharge of water and contaminants, via seepage or surface runoff, from topsoil and brown rock stockpiles, the TSF, various ELFs, the Shepherds Service Corridor, haul roads, erosion and sediment control structures and treatment devices, two aggregate pits and other ancillary mining development, operation and maintenance activities; 
The discharge of water and contaminants from erosion and sediment control structures in accordance with certified Site-Specific Erosion and Sediment Control Plans; 
The discharge of water and contaminants within a 100 m setback from natural inland wetlands, including where the discharge may enter a wetland and change its water level range or hydrological function; and
The discharge of water for dust suppression purposes;
within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	





	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.

	General

	3
	All roofs and potentially small, impervious car parking areas within the Project Site associated with offices and administration buildings and vehicle servicing and repair areas shall be connected to a reticulated stormwater system.





	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S15
	A Discharge Permit to discharge contaminants into or onto land, including in circumstances where it may enter water, associated with the discharge of tailings into the TSF within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One).

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.





	CONSENT TYPE AND ACTIVITY AUTHORISED
	RMA S15
	A Discharge Permit to discharge contaminants to air from the crushing and screening of aggregates, and mining operations (including mineral extraction and processing activities) associated with the BOGP within the Project Site shown on Plan 1 - Project Overview Plan annexed as part of Attachment 1 – Plans to the Common Conditions (Schedule One). 

	TERM
	35 years
	

	LAPSE PERIOD
	10 years
	



	No.
	Condition

	Schedule One – Common Conditions Which Apply to All Otago Regional Council and Central Otago District Council Consents

	1
	The Consent Holder must comply with the Common Conditions in Schedule One (which apply to all of the consents for the BOGP within the jurisdiction of the Central Otago District Council and the Otago Regional Council) to the extent relevant to the management of activities authorised by this consent.

	Schedule Two – General Conditions Which Apply to All Otago Regional Council Consents

	2
	The Consent Holder must comply with the General Conditions in Schedule Two (which apply to all of the consents for the BOGP within the jurisdiction of the Otago Regional Council) to the extent relevant to the activities authorised by this consent.




SCHEDULE ONE
BENDIGO-OPHIR GOLD PROJECT - COMMON CONDITIONS WHICH APPLY TO ALL OF THE RESOURCE CONSENTS WITHIN THE JURISDICTION OF THE CENTRAL OTAGO DISTRICT COUNCIL AND OTAGO REGIONAL COUNCIL 


SCHEDULE TWO
BENDIGO-OPHIR GOLD PROJECT - GENERAL CONDITIONS WHICH APPLY TO ALL OF THE RESOURCE CONSENTS WITHIN THE JURISDICTION OF THE OTAGO REGIONAL COUNCIL

	Bendigo-Ophir Gold Project – Proposed Conditions for the Otago Regional Council Consents
	2
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