	
	
	



APPENDIX 8 
Waimakariri District Council’s comments on proposed conditions for the Resource consent Requirement to disturb contaminated land
Part B: Waimakariri District Council Resource Consent
The resource consent identified below is sought to allow the Consent Holder to construct the State Highway 1 North Canterbury—Woodend Bypass Project (Belfast to Pegasus): 
	Ref
	Consent type and scope

	NES-CS
	Land use consent
Disturbance and excavation of contaminated soil and material to which the NES-CS applies, for the purposes of constructing the State Highway 1 North Canterbury—Woodend Bypass Project (Belfast to Pegasus).


Note: The proposed conditions in Part B pertain only to the management of environmental effects falling under the jurisdiction of WDC under the Resource Management (National Environmental Standard for Assessing and Managing Contaminants in Soil to Protect Human Health) Regulations 2011.  For the management of other effects falling under the jurisdiction of WDC, please refer to the conditions of the existing designation (Volume 2B) and the alterations sought (Volume 2C).
Definitions and terms used in this resource consent
	Abbreviation/term
	Meaning

	CSMP
	Contaminated Sites Management Plan

	Consent Holder
	NZ Transport Agency Waka Kotahi

	NES-CS
	Resource Management (National Environmental Standard for Managing Contaminants in Soil to Protect Human Health) Regulations 2011

	Project
	State Highway 1 North Canterbury – Woodend Bypass Project (Belfast to Pegasus) (the construction, operation, and maintenance thereof)

	Site
	The land contained within the area delineated as “Project Site” in Volume 4C of the Application.

	SQP 
	Suitably Qualified Person: A person (or persons) who are competent and experienced in the field of expertise that is relevant to a particular task or action directed by a condition.

	WDC
	Waimakariri District Council

	Working Day
	A day of the week other than—
(a)	a Saturday, a Sunday, Waitangi Day, Good Friday, Easter Monday, Anzac Day, the Sovereign’s birthday, Te Rā Aro ki a Matariki/Matariki Observance Day, and Labour Day; and
(b)	if Waitangi Day or Anzac Day falls on a Saturday or a Sunday, the following Monday; and
(c)	a day in the period commencing on 20 December in any year and ending with 10 January in the following year.




Conditions
The following table outlines the conditions proposed by NZTA and proposed changes/additions by WDC: 

	Ref
	Condition
	NZTA Comments 
	WDC comments 

	Scope and General
	
	

	NES-CS.1
	This resource consent shall lapse 10 years from the date of commencement of the consents in accordance with section 97 of the FTAA.
	
	

	2
	WDC shall be notified of the commencement of earthworks 5 days prior to their commencement on a contaminated site.
	
	A new condition is recommended 

	NES-CS.32
	WDC may serve notice on the Consent Holder under section 128(1) of the Act of its intention to review the conditions of thisese resource consents at any time within six months of the first, second, third, fourth, and fifth anniversaries of the date of Commencement of Construction Works, and thereafter five yearly.  The purpose of such a review is to deal with any adverse effect on the environment which may result from the consented activities and which it is appropriate to deal with at a later stage. Any review under this condition must give effect to the purpose of the Fast-track Approvals Act 2024.
	
	

	Further investigation 
	
	

	NES-CS.43
	The further investigation requirements outlined in the Ground Contamination Investigation Report for HAIL sites which have not yet been investigated (Volume 3F of the Substantive Application Prepared by Tonkin Taylor dated November 2025 saved in WDC records TRIM 260107001866, 260107001868 and 260107001868) shall be completed prior to earthworks commencing in the respective area. Investigation works shall be completed by a SQPSQP and shall be provided to WDC for  approval prior to earthworks commencing..  
	
	Additional information added to ensure correct references to application information and include WDC approval requirement. 

	Remediation and validation
	
	

	NES-CS.5X
	Where contamination is identified at concentrations requiring active remediation, 
works shall be undertaken in accordance with a site-specific Remedial Action Plan (RAP). Active remediation is defined as the requirement to address unacceptable concentrations of contaminants due to risks to human health that would not otherwise be addressed through construction works.
The RAP must be provided to Waimakariri District Council, Attention:  Compliance Manager for approval


The RAP must include:
-	Remedial objectives and targets
-	Remedial methodology 
-	Any additional controls required to manage contamination discharges during remediation works 
-	Any validation sampling or methodologies that will be undertaken to demonstrate successful completion of the remedial works
	Additional condition to ensure the CRC and NESCS sets are aligned.  
	

	NES-CS.6X
	
Within 2 months of the completion of any remediation works required under NES-CS.X a Site Validation Report (SVR) must be prepared by a SQP in accordance with the Ministry for Environment’s Contaminated Land Management Guidelines No 1 - Reporting on Contaminated Sites in New Zealand to validate whether the objectives of the RAP have been achieved. 

The SVR must be provided to Waimakariri District Council, Attention:  Compliance Manager.

The SVR must include the following information: 
a.	Summary of remediation works undertaken.
b.	Confirmation the remediation objectives and targets have been successfully achieved, including validation sampling (if required) or documentation of validation methodologies.  
c.	Details of any ongoing site management where contamination remains in place. 
d.	Evidence of the fate of material removed from the site.
	Additional condition to ensure the CRC and NESCS sets are aligned. 

	

	Contaminated Sites Management Plan
	
	

	NES-CS.74
	All Project earthworks, including the reuse of soil within the Site, shall be undertaken in 
accordance with the Contaminated Site Management Plan (CSMP) required under 
resource consent CRCXXXXXX [insert ref] (Consent C1).
	
	The reference to ECAN consent will be outside of the scope of this consent. 


	Works Completion Report 
	
	

	NES-CS.85
	Within 2 months of the completion of the soil disturbance authorised under this resource consent (or if relevant, within 2 months of completion of the soil disturbance of a Project stage), the Consent Holder shall provide a Works Completion Report. (WCR). The purpose of the WCR is to demonstrate that the works were carried out in accordance with the requirements of the CSMP. The report shall be prepared by a SQP. The Works Completion Report shall include:
(a) A summary of the works undertaken, including dates of commencement and completion;
(b) Details of any unexpected contamination encountered during the works and the response to such findings;
(c) A summary of all soil sampling and analysis results, including comparison with relevant soil contaminant standards;
(d) Records of soil disposal, including volumes, destinations, and waste acceptance documentation for any soil removed from the site;
(e) Confirmation that the site is suitable for the intended use (or otherwise specify any ongoing management requirements);
(f) Any recommendations for further monitoring, remediation, or site management if applicable;
(g) Photographic evidence of the works undertaken.
(h) Details of the reuse or disposal of contaminated soil within the site.
If remedial actions are required, the Works Completion Report shall summarise the remediation works undertaken and validated.
	
	

	NES-CS.9
	Where any contamination above applicable soil contaminant standards will be retained or managed on site, a Long Term Site Management Plan shall be submitted to WDC, Attention: Compliance Manager within two months of completing the construction works. The Long Term Site Management Plan shall include:
a.	Confirmation that the construction works  have been completed and were carried out in accordance with the SMP
b.	Details of any soil sampling and validation carried out
c.	Accurate details of the location and extent of any encapsulated soils, including an estimate of the volume of material discharged; and
d.	Details of the future management of any encapsulated soils, including how the integrity of the lining or seal will be maintained and monitored over time”
	
	Additional condition is recommended 

	
	Contamination Discovery
	
	

	NES-CS.10
	
In the event of contamination discovery e.g., visible staining, odours, and/or other conditions that indicate soil contamination, then work must cease until a Suitably Qualified and Experienced Practitioner (SQEP) has assessed the matter and advised of the appropriate remediation and/or disposal options for these soils. Any measures to manage the risk from potential soil contamination must be approved by the Waimakariri District Council. Attention:  Compliance Manager 
 

	
	New condition is recommended 
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